* **Telaio**

Lumen eRIDE Carbon HMX  
Integrated Suspension Technology  
Flex Pivot / Adjustable head angle  
Syncros Cable Integration System  
TQ HPR50 / UDH Interface / 12x148mm with 55mm Chainline

* **Escursione**

Front: 130mm / Rear: 130mm

* **Forcella**

FOX 34 Float Rhythm Air Grip  
3-Modes / Kabolt 15x110mm axle / tapered steerer  
44mm offset / Reb. Adj. / Lockout / 130mm travel

* **Ammortizzatore posteriore**

FOX NUDE 5T EVOL Trunnion  
SCOTT custom w. travel / geo adj.  
3 modes: Lockout-Traction Control-Descend  
Custom large Air volume / DPS / Reb. Adj.  
Travel 130-90-Lockout / T165X45mm

* **comando remoto**

SCOTT TwinLoc Suspension System  
3 modes front and rear / integ. Grip clamp

* **Motore**

TQ HPR50 Mid Motor drive 50Nm max Torque / EU: 25kmh / US: 20mph

* **Batteria**

TQ Internal 360Wh

* **Schermo**

TQ HPR  
Bluetooth / ANT+ / Dedicated Smartphone app

* **Caricatore**

TQ 100-240V-4A

* **Deragliatore posteriore**

Shimano XT RD-M8100 SGS  
Shadow Plus / 12 Speed

* **Leve del cambio**

Shimano Deore SL-M6100-IR / Rapidfire Plus  
Ispec EV clamp

* **Guarnitura**

FSA Alloy crankset / 175mm / 34T

* **Guidacatena**

e\*thirteen / e\*spec Slider

* **Corona**

Scott custom spider / FSA 12Speed 34T chainring

* **Catena**

Shimano CN-M6100

* **Cassetta**

Shimano CS-M6100 / 10-51 T

* **Freni**

Shimano Deore M6120 4 Piston Disc

* **Disco del freno**

Front: SM-RT64 CL 180mm / Rear: RT-EM600 CL 180mm

* **Manubrio**

Syncros Fraser 2.0 DC Alloy 6061 D.B.  
mini Rise / back sweep 8° / 760mm  
Syncros Performance XC lock-on grips

* **Attacco manubrio**

Syncros DC 2.0  
Syncros Cable Integration System  
0° rise / 6061 Alloy / 31.8mm / 1 1/8"

* **Reggisella**

Syncros Duncan Dropper Post 2.0  
31.6mm / S & M size 125mm / L size 150mm / XL size 170mm

* **Sella**

Syncros Tofino 1.5 Regular, Titanium rails

* **Serie sterzo**

Syncros - Acros Angle adjust & Cable Routing HS System  
+-0.6° head angle adjustment  
ZS56/28.6 – ZS56/40 MTB

* **Mozzo anteriore**

Formula CL-811 / 15x110mm

* **Mozzo posteriore**

Formula CL-148M / 12x148mm / Micro Spline  
Syncros Axle w/Removable Lever  
with 6mm Allen, T30 and T25 Tools

* **Raggi**

Stainless Black 15G / 1.8mm

* **Cerchio**

Syncros X-30SE / 32H / 30mm  
Tubeless ready

* **Gomma anteriore**

Schwalbe Wicked Will 29x2.4" EVO  
Super Race / TLE / 67EPI / Addix Speed Soft

* **Gomma posteriore**

Schwalbe Wicked Will 29x2.4" EVO  
Super Race / TLE / 67EPI / Addix Speed Grip

* **Peso in kg (approx.)**

17.6 (Tubeless setup)

* **Peso in lbs (approx.)**

38.8 (Tubeless setup)

* **Peso totale**

128kg  
Il peso totale include la bici, il ciclista, l'equipaggiamento, e potenzialmente bagagli aggiuntivi